(footprint "TO-72-4" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "REF**" (at 2.8448 4.064 unlocked) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.1)))
    (tstamp 7bc3454f-7039-4b2c-817d-1689a2866672)
  )
  (fp_text value "TO-72-4" (at 0 1 unlocked) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    (tstamp 21e4b5f6-262b-4e6f-84ea-d342a3a8667d)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "B.Fab")
      (effects (font (size 1 1) (thickness 0.15)) (justify mirror))
    (tstamp 65f87474-fc03-44bd-95a6-0b5a9c27787f)
  )
  (fp_line (start 1.6002 -2.1336) (end 2.245769 -2.773922)
    (stroke (width 0.127) (type default)) (layer "F.SilkS") (tstamp f38d3836-c6f1-495b-adda-32a62f50fc62))
  (fp_line (start 2.222788 -1.473806) (end 2.883188 -2.134206)
    (stroke (width 0.127) (type default)) (layer "F.SilkS") (tstamp 0be54588-7b9f-4a3f-b09e-c5907b7bd767))
  (fp_line (start 2.245769 -2.773922) (end 2.883188 -2.134206)
    (stroke (width 0.127) (type solid)) (layer "F.SilkS") (tstamp a0ff98f8-cb7b-4107-93ce-7a8c80a33c17))
  (fp_arc (start 2.222788 -1.473806) (mid -1.939741 1.830362) (end 1.6002 -2.1336)
    (stroke (width 0.127) (type default)) (layer "F.SilkS") (tstamp 16648624-d0c0-43ef-ba23-ebcffc837aff))
  (fp_circle (center 0 0) (end 2.45 0)
    (stroke (width 0.05) (type default)) (fill none) (layer "Edge.Cuts") (tstamp a4c506fb-3e5a-4733-8c1a-a960c7c94b43))
  (fp_rect (start 5.08 5.08) (end -5.08 -5.08)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp eaf1a88a-9763-4c4f-947f-3f648149a92a))
  (pad "1" thru_hole oval (at 4 0) (size 1.6 1.2) (drill 0.7) (layers "*.Cu" "*.Mask") (tstamp 210d5c37-058d-430a-9b24-cbf3f53f4d4d))
  (pad "2" thru_hole oval (at 0 4) (size 1.2 1.6) (drill 0.7) (layers "*.Cu" "*.Mask") (tstamp a80ff633-4d74-45b8-83d6-43f050282b44))
  (pad "3" thru_hole oval (at -4 0) (size 1.6 1.2) (drill 0.7) (layers "*.Cu" "*.Mask") (tstamp fdb3a972-b987-491f-8863-846a25e9c772))
  (pad "4" thru_hole oval (at 0 -4) (size 1.2 1.6) (drill 0.7) (layers "*.Cu" "*.Mask") (tstamp 85fc4462-4582-4a58-baaf-5930e60c3c04))
)
