(export (version D)
  (design
    (source /home/trefin/Downloads/X8.5DMM/10V-DLTZ/10V-DLTZ.sch)
    (date "Sun 14 Nov 2021 11:13:29 PM CET")
    (tool "Eeschema 5.1.5+dfsg1-2build2")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source 10V-DLTZ.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref SZ1)
      (value LTZ1000)
      (libsource (lib CustSymbols) (part LTZ1000) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 618C50A4))
    (comp (ref U5)
      (value NE555)
      (libsource (lib CustSymbols) (part NE555) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 618C9381))
    (comp (ref R3)
      (value 1K)
      (libsource (lib CustSymbols) (part RES) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 618D15B0))
    (comp (ref R4)
      (value 619K)
      (libsource (lib CustSymbols) (part RES) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 618D20CC))
    (comp (ref C4)
      (value Capacitor)
      (libsource (lib CustSymbols) (part Capacitor) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 618D4A1B))
    (comp (ref C3)
      (value 10nF)
      (libsource (lib CustSymbols) (part Capacitor) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 618D5EE9))
    (comp (ref C5)
      (value Capacitor)
      (libsource (lib CustSymbols) (part Capacitor) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 618E42BF))
    (comp (ref C6)
      (value 47uF)
      (libsource (lib CustSymbols) (part Capacitor) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 618E4C7E))
    (comp (ref C1)
      (value 150p)
      (libsource (lib CustSymbols) (part Capacitor) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 6190664A))
    (comp (ref U3)
      (value DAC08)
      (libsource (lib CustSymbols) (part DAC08) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 619121FB))
    (comp (ref R5)
      (value 1K)
      (libsource (lib CustSymbols) (part RES) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 61938992))
    (comp (ref R2)
      (value 2K)
      (libsource (lib CustSymbols) (part RES) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 619507A7))
    (comp (ref U2)
      (value ADA4523-1)
      (libsource (lib CustSymbols) (part ADA4523-1) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 61951849))
    (comp (ref R1)
      (value 2K)
      (libsource (lib CustSymbols) (part RES) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 6196E698))
    (comp (ref U1)
      (value ADA4523-1)
      (libsource (lib CustSymbols) (part ADA4523-1) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 6196E69E))
    (comp (ref C2)
      (value 150p)
      (libsource (lib CustSymbols) (part Capacitor) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 619895E0))
    (comp (ref U4)
      (value SN74HC590A)
      (libsource (lib CustSymbols) (part SN74HC590A) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 618ECB41))
    (comp (ref Rn1)
      (value NOMC1603)
      (libsource (lib CustSymbols) (part NOMC1603) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 61920C9C))
    (comp (ref Rn2)
      (value NOMC1603)
      (libsource (lib CustSymbols) (part NOMC1603) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 61927A48)))
  (libparts
    (libpart (lib CustSymbols) (part ADA4523-1)
      (fields
        (field (name Reference) U)
        (field (name Value) ADA4523-1))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name -) (type input))
        (pin (num 3) (name +) (type input))
        (pin (num 4) (name ~) (type power_in))
        (pin (num 6) (name ~) (type output))
        (pin (num 7) (name ~) (type power_in))
        (pin (num 8) (name ~) (type input))))
    (libpart (lib CustSymbols) (part Capacitor)
      (fields
        (field (name Reference) C)
        (field (name Value) Capacitor))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name ~) (type input))))
    (libpart (lib CustSymbols) (part DAC08)
      (fields
        (field (name Reference) U)
        (field (name Value) DAC08))
      (pins
        (pin (num 1) (name VCC) (type passive))
        (pin (num 2) (name VR+) (type passive))
        (pin (num 3) (name VR-) (type passive))
        (pin (num 4) (name CMP) (type passive))
        (pin (num 5) (name Vlc) (type passive))
        (pin (num 6) (name /IOUT) (type passive))
        (pin (num 7) (name V-) (type passive))
        (pin (num 8) (name Iout) (type passive))
        (pin (num 9) (name B1) (type passive))
        (pin (num 10) (name B2) (type passive))
        (pin (num 11) (name B3) (type passive))
        (pin (num 12) (name B4) (type passive))
        (pin (num 13) (name B5) (type passive))
        (pin (num 14) (name B6) (type passive))
        (pin (num 15) (name B7) (type passive))
        (pin (num 16) (name B8) (type passive))))
    (libpart (lib CustSymbols) (part LTZ1000)
      (fields
        (field (name Reference) SZ)
        (field (name Value) LTZ1000))
      (pins
        (pin (num 1) (name ~) (type input))
        (pin (num 2) (name ~) (type input))
        (pin (num 3) (name ~) (type input))
        (pin (num 4) (name ~) (type input))
        (pin (num 5) (name ~) (type input))
        (pin (num 6) (name ~) (type input))
        (pin (num 7) (name ~) (type input))
        (pin (num 8) (name ~) (type input))))
    (libpart (lib CustSymbols) (part NE555)
      (fields
        (field (name Reference) U)
        (field (name Value) NE555))
      (pins
        (pin (num 1) (name GND) (type input))
        (pin (num 2) (name TRG) (type input))
        (pin (num 3) (name OUT) (type input))
        (pin (num 4) (name RST) (type input))
        (pin (num 5) (name CNT) (type input))
        (pin (num 6) (name TRS) (type input))
        (pin (num 7) (name DCH) (type input))
        (pin (num 8) (name VCC) (type input))))
    (libpart (lib CustSymbols) (part NOMC1603)
      (fields
        (field (name Reference) Rn)
        (field (name Value) NOMC1603))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive))
        (pin (num 9) (name ~) (type passive))
        (pin (num 10) (name ~) (type passive))
        (pin (num 11) (name ~) (type passive))
        (pin (num 12) (name ~) (type passive))
        (pin (num 13) (name ~) (type passive))
        (pin (num 14) (name ~) (type passive))
        (pin (num 15) (name ~) (type passive))
        (pin (num 16) (name ~) (type passive))))
    (libpart (lib CustSymbols) (part RES)
      (fields
        (field (name Reference) R)
        (field (name Value) RES))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib CustSymbols) (part SN74HC590A)
      (fields
        (field (name Reference) U)
        (field (name Value) SN74HC590A))
      (pins
        (pin (num 1) (name QB) (type passive))
        (pin (num 2) (name QC) (type passive))
        (pin (num 3) (name QD) (type passive))
        (pin (num 4) (name QE) (type passive))
        (pin (num 5) (name QF) (type passive))
        (pin (num 6) (name QG) (type passive))
        (pin (num 7) (name QH) (type passive))
        (pin (num 8) (name GND) (type passive))
        (pin (num 9) (name /RCO) (type passive))
        (pin (num 10) (name /CCLR) (type passive))
        (pin (num 11) (name CCLK) (type passive))
        (pin (num 12) (name /CKEN) (type passive))
        (pin (num 13) (name RCLK) (type passive))
        (pin (num 14) (name /OE) (type passive))
        (pin (num 15) (name QA) (type passive))
        (pin (num 16) (name VCC) (type passive)))))
  (libraries
    (library (logical CustSymbols)
      (uri /home/trefin/Downloads/X8.5DMM/10V-DLTZ/CustSymbols.lib)))
  (nets
    (net (code 1) (name "Net-(U4-Pad9)")
      (node (ref U4) (pin 9)))
    (net (code 2) (name GNDD)
      (node (ref U4) (pin 12))
      (node (ref U4) (pin 13))
      (node (ref U4) (pin 14))
      (node (ref U4) (pin 8))
      (node (ref C4) (pin 2))
      (node (ref U5) (pin 1))
      (node (ref C3) (pin 2))
      (node (ref C5) (pin 2))
      (node (ref C6) (pin 2)))
    (net (code 3) (name "Net-(Rn1-Pad3)")
      (node (ref Rn1) (pin 5))
      (node (ref SZ1) (pin 5))
      (node (ref Rn1) (pin 7))
      (node (ref Rn1) (pin 3)))
    (net (code 4) (name "Net-(Rn1-Pad11)")
      (node (ref Rn1) (pin 13))
      (node (ref Rn1) (pin 16))
      (node (ref Rn1) (pin 11))
      (node (ref Rn1) (pin 9)))
    (net (code 5) (name "Net-(Rn2-Pad1)")
      (node (ref Rn2) (pin 1)))
    (net (code 6) (name "Net-(Rn2-Pad11)")
      (node (ref Rn2) (pin 11))
      (node (ref Rn2) (pin 14)))
    (net (code 7) (name "Net-(U3-Pad13)")
      (node (ref U3) (pin 13)))
    (net (code 8) (name "Net-(U3-Pad12)")
      (node (ref U3) (pin 12)))
    (net (code 9) (name "Net-(U3-Pad11)")
      (node (ref U3) (pin 11)))
    (net (code 10) (name "Net-(U3-Pad10)")
      (node (ref U3) (pin 10)))
    (net (code 11) (name "Net-(U3-Pad9)")
      (node (ref U3) (pin 9)))
    (net (code 12) (name Clk)
      (node (ref U5) (pin 3)))
    (net (code 13) (name +5V)
      (node (ref R3) (pin 1))
      (node (ref U5) (pin 4))
      (node (ref U5) (pin 8))
      (node (ref U4) (pin 16))
      (node (ref U4) (pin 10)))
    (net (code 14) (name "Net-(Rn2-Pad12)")
      (node (ref Rn2) (pin 13))
      (node (ref Rn2) (pin 12)))
    (net (code 15) (name B0)
      (node (ref U4) (pin 1)))
    (net (code 16) (name "Net-(U4-Pad11)")
      (node (ref U4) (pin 11)))
    (net (code 17) (name LSB)
      (node (ref U4) (pin 15)))
    (net (code 18) (name B1)
      (node (ref U4) (pin 2)))
    (net (code 19) (name B2)
      (node (ref U4) (pin 3)))
    (net (code 20) (name B3)
      (node (ref U4) (pin 4)))
    (net (code 21) (name B4)
      (node (ref U4) (pin 5)))
    (net (code 22) (name B5)
      (node (ref U4) (pin 6)))
    (net (code 23) (name DONE)
      (node (ref U4) (pin 7)))
    (net (code 24) (name "Net-(Rn1-Pad10)")
      (node (ref Rn1) (pin 15))
      (node (ref Rn1) (pin 14))
      (node (ref Rn1) (pin 12))
      (node (ref Rn1) (pin 10)))
    (net (code 25) (name "Net-(Rn1-Pad4)")
      (node (ref SZ1) (pin 8))
      (node (ref Rn1) (pin 4))
      (node (ref Rn1) (pin 6))
      (node (ref Rn1) (pin 8)))
    (net (code 26) (name "Net-(Rn2-Pad6)")
      (node (ref Rn2) (pin 6))
      (node (ref Rn2) (pin 7)))
    (net (code 27) (name "Net-(Rn2-Pad15)")
      (node (ref Rn2) (pin 15))
      (node (ref Rn2) (pin 16)))
    (net (code 28) (name "Net-(Rn2-Pad2)")
      (node (ref Rn2) (pin 3))
      (node (ref Rn2) (pin 2)))
    (net (code 29) (name "Net-(Rn2-Pad4)")
      (node (ref Rn2) (pin 4))
      (node (ref Rn2) (pin 5)))
    (net (code 30) (name "Net-(Rn1-Pad1)")
      (node (ref Rn1) (pin 2))
      (node (ref Rn2) (pin 8))
      (node (ref Rn1) (pin 1)))
    (net (code 31) (name "Net-(Rn2-Pad10)")
      (node (ref Rn2) (pin 10))
      (node (ref Rn2) (pin 9)))
    (net (code 32) (name "Net-(C4-Pad1)")
      (node (ref U5) (pin 6))
      (node (ref U5) (pin 2))
      (node (ref R4) (pin 2))
      (node (ref C4) (pin 1)))
    (net (code 33) (name "Net-(C5-Pad1)")
      (node (ref C5) (pin 1))
      (node (ref C6) (pin 1)))
    (net (code 34) (name "Net-(C3-Pad1)")
      (node (ref C3) (pin 1))
      (node (ref U5) (pin 5)))
    (net (code 35) (name "Net-(C1-Pad2)")
      (node (ref R1) (pin 2))
      (node (ref U1) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref U3) (pin 6)))
    (net (code 36) (name "Net-(U3-Pad1)")
      (node (ref U3) (pin 1)))
    (net (code 37) (name "Net-(SZ1-Pad2)")
      (node (ref SZ1) (pin 2)))
    (net (code 38) (name "Net-(SZ1-Pad3)")
      (node (ref SZ1) (pin 3)))
    (net (code 39) (name "Net-(SZ1-Pad4)")
      (node (ref SZ1) (pin 4)))
    (net (code 40) (name "Net-(SZ1-Pad6)")
      (node (ref SZ1) (pin 6)))
    (net (code 41) (name "Net-(SZ1-Pad7)")
      (node (ref SZ1) (pin 7)))
    (net (code 42) (name "Net-(R3-Pad2)")
      (node (ref U5) (pin 7))
      (node (ref R4) (pin 1))
      (node (ref R3) (pin 2)))
    (net (code 43) (name "Net-(C2-Pad2)")
      (node (ref U2) (pin 2))
      (node (ref R2) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref U3) (pin 8)))
    (net (code 44) (name "Net-(U1-Pad3)")
      (node (ref U1) (pin 3)))
    (net (code 45) (name "Net-(U1-Pad4)")
      (node (ref U1) (pin 4)))
    (net (code 46) (name "Net-(U1-Pad7)")
      (node (ref U1) (pin 7)))
    (net (code 47) (name "Net-(U1-Pad8)")
      (node (ref U1) (pin 8)))
    (net (code 48) (name "Net-(C1-Pad1)")
      (node (ref C1) (pin 1))
      (node (ref R1) (pin 1))
      (node (ref U1) (pin 6)))
    (net (code 49) (name "Net-(U3-Pad14)")
      (node (ref U3) (pin 16))
      (node (ref U3) (pin 15))
      (node (ref U3) (pin 14)))
    (net (code 50) (name "Net-(R5-Pad2)")
      (node (ref R5) (pin 2)))
    (net (code 51) (name "Net-(U3-Pad2)")
      (node (ref U3) (pin 2)))
    (net (code 52) (name "Net-(U3-Pad3)")
      (node (ref U3) (pin 3)))
    (net (code 53) (name "Net-(U3-Pad4)")
      (node (ref U3) (pin 4)))
    (net (code 54) (name "Net-(U3-Pad5)")
      (node (ref U3) (pin 5)))
    (net (code 55) (name "Net-(U3-Pad7)")
      (node (ref U3) (pin 7)))
    (net (code 56) (name "Net-(R5-Pad1)")
      (node (ref R5) (pin 1)))
    (net (code 57) (name "Net-(SZ1-Pad1)")
      (node (ref SZ1) (pin 1)))
    (net (code 58) (name "Net-(C2-Pad1)")
      (node (ref U2) (pin 6))
      (node (ref R2) (pin 1))
      (node (ref C2) (pin 1)))
    (net (code 59) (name "Net-(U2-Pad1)")
      (node (ref U2) (pin 1)))
    (net (code 60) (name "Net-(U2-Pad3)")
      (node (ref U2) (pin 3)))
    (net (code 61) (name "Net-(U2-Pad4)")
      (node (ref U2) (pin 4)))
    (net (code 62) (name "Net-(U2-Pad7)")
      (node (ref U2) (pin 7)))
    (net (code 63) (name "Net-(U2-Pad8)")
      (node (ref U2) (pin 8)))
    (net (code 64) (name "Net-(U1-Pad1)")
      (node (ref U1) (pin 1)))))